Install & Build
===============
0. Introduction
   This file will show you how to build the RTL865x linux system. Besides, It
will guide you how to download the built image to Realtek EV (Evaluation)
board for testing. PLEASE NOTE, the download image will overwrite the original
image existed in the flash memory of EV board.

1. Build Environment
   RedHat 7.3/9.0

2. Install Toolchain
    - mkdir -p /toolchain
    - tar xvfz rtl865x-toolchain-1.3.6.tar.gz -C /toolchain
    - export PATH=/toolchain/rsdk/linux:$PATH
	(you can add the path in your ~/.bash_profile)

3. Build Linux kernel
   - tar zxvf DAP-1360-GPL.tar.gz
   - cd ./dev_1.2f_102B01/rtl865x-linux-1.2f/linux-2.4.18
   - ./mk

4. Make a firmware image
   - cd ./dev_1.2f_102B01/rtl865x-linux-1.2f/AP
   - 'make gw' will build the root file system for gw platform
   - ==> 'image.bin' is the firmware image 
   	  
